How to program the voltage?

• Need adjustable voltage source.

1) set the minimum measured voltage (from 6 v) at the source

2) press the button and connect the indicator, start to blink two red diodes (entered into programming mode)

3) release the button, blinks the minimum voltage diode.

4) short press the button (keep the minimum voltage)-light up two red diodes and blinks blue.

5) put on the source the maximum measured voltage, briefly press the button (keep the maximum voltage) will light up all the leds.

6) power off (programming is over). The controller itself will break the entire range of voltages in accordance with the percentage of the battery charge.