**48-84V 45А универсален със/без сензорен контролер**

Thanks delivered quickly perfectly. checked the controller works perfectly, powerful, feel the difference before other ct 35a controller. There was a misunderstanding with the controller setup (the seller explained everything, thanks to him). tell those who first try to configure the controller, (immediately mark the controller is able to work without lcd display): connect phase wires, hall, gas, battery, then connect two white wires, then lock the wire or anything wire :( ignition) And the motor should spin if it turns to the right side (i.e. forward), you can disconnect two white wires and leave the jumper on the wire :( ignition), (note if the jumper on this wire remove, then the trigger of gas will not work). If the motor turns back then repeat it again.